<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<text>By Tonnerre33</text>
<text>MySensors</text>
<text>V1.1.3</text>
<text>AVRISP</text>
<text>Compatible</text>
<text>+</text>
<wire x1="55" y1="0" x2="35" y2="0" width="0" layer="20"/>
<wire x1="0" y1="5" x2="0" y2="24" width="0" layer="20"/>
<wire x1="0" y1="24" x2="55" y2="24" width="0" layer="20"/>
<wire x1="55" y1="24" x2="55" y2="0" width="0" layer="20"/>
<hole x="3" y="22" drill="3.5"/>
<hole x="3" y="7" drill="3.5"/>
<wire x1="0" y1="5" x2="30" y2="5" width="0" layer="20"/>
<wire x1="30" y1="5" x2="35" y2="0" width="0" layer="20"/>
<text>FTDI</text>
<text>+</text>
</plain>
<libraries>
<library name="LowPowerLab">
<packages>
<package name="0805-CAP">
</package>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="0805-RES">
</package>
<package name="0805-LED">
</package>
</packages>
</library>
<library name="rollershutter">
<packages>
<package name="NRF24L01+SMD_MODULE">
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="RESONATOR-SMD">
</package>
<package name="TACTILE-SWITCH-1101NE">
<description>Sparkfun SKU# COM-08229</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<packages>
<package name="1X06-1MM">
<description>Works with part #579 (https://www.sparkfun.com/products/579). Commonly used on GPS modules EM408, EM406 and GP-635T. Also compatible with cable 9123 (https://www.sparkfun.com/products/9123) and cable 574 (https://www.sparkfun.com/products/574).</description>
</package>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="JRS-CR123-BatteryHolder">
<packages>
<package name="CR123_BATTERYHOLDER">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="LowPowerLab" package="0805-CAP" value="100n"/>
<element name="C2" library="LowPowerLab" package="0805-CAP" value="100n"/>
<element name="IC1" library="LowPowerLab" package="TQFP32-08" value="ATMEGA328P"/>
<element name="R1" library="LowPowerLab" package="0805-RES" value="1k5"/>
<element name="R2" library="LowPowerLab" package="0805-RES" value="10k"/>
<element name="R3" library="LowPowerLab" package="0805-RES" value="1k5"/>
<element name="SL2" library="SparkFun-Connectors" package="1X06-1MM" value=""/>
<element name="SL3" library="SparkFun-Connectors" package="1X06-1MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="LowPowerLab" package="0805-LED" value=""/>
<element name="D1" library="LowPowerLab" package="0805-LED" value=""/>
<element name="RF1" library="rollershutter" package="NRF24L01+SMD_MODULE" value="NRF24L01+SMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="LowPowerLab" package="0805-RES" value="56k"/>
<element name="C3" library="LowPowerLab" package="0805-CAP" value="4u7"/>
<element name="U$3" library="SparkFun" package="RESONATOR-SMD" value="8MHZ"/>
<element name="RESET" library="SparkFun" package="TACTILE-SWITCH-1101NE" value="-"/>
<element name="C4" library="LowPowerLab" package="0805-CAP" value="0.1uF"/>
<element name="J1" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="LED1" library="led" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="LowPowerLab" package="0805-RES" value="1k5"/>
<element name="U$1" library="JRS-CR123-BatteryHolder" package="CR123_BATTERYHOLDER" value=""/>
<element name="R6" library="LowPowerLab" package="0805-RES" value="1M"/>
<element name="R7" library="LowPowerLab" package="0805-RES" value="470k"/>
<element name="C5" library="LowPowerLab" package="0805-CAP" value="0.1uF"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="D2" pad="PLUS"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="21"/>
<contactref element="D2" pad="MINUS"/>
<contactref element="SL2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="RF1" pad="GND"/>
<contactref element="U$3" pad="2"/>
<contactref element="RESET" pad="P$2"/>
<contactref element="D1" pad="MINUS"/>
<contactref element="LED1" pad="K"/>
<contactref element="U$1" pad="GND"/>
<contactref element="R7" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="SL3" pad="2"/>
<contactref element="SL3" pad="3"/>
</signal>
<signal name="RST">
<contactref element="R2" pad="1"/>
<contactref element="IC1" pad="29"/>
<contactref element="C1" pad="2"/>
<contactref element="SL2" pad="4"/>
<contactref element="RESET" pad="P$1"/>
</signal>
<signal name="VCC">
<contactref element="R2" pad="2"/>
<contactref element="IC1" pad="18"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="6"/>
<contactref element="SL2" pad="1"/>
<contactref element="RF1" pad="3V"/>
<contactref element="R4" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="U$1" pad="VCC"/>
<contactref element="R6" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="SL3" pad="1"/>
</signal>
<signal name="DTR">
<contactref element="C1" pad="1"/>
<contactref element="SL3" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="12"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="R3" pad="1"/>
<contactref element="D1" pad="PLUS"/>
</signal>
<signal name="MISO">
<contactref element="SL2" pad="3"/>
<contactref element="IC1" pad="16"/>
<contactref element="RF1" pad="MISO"/>
</signal>
<signal name="MOSI">
<contactref element="SL2" pad="5"/>
<contactref element="IC1" pad="15"/>
<contactref element="RF1" pad="MOSI"/>
</signal>
<signal name="SCK">
<contactref element="SL2" pad="6"/>
<contactref element="IC1" pad="17"/>
<contactref element="R1" pad="2"/>
<contactref element="RF1" pad="SCK"/>
</signal>
<signal name="D0_RX">
<contactref element="SL3" pad="5"/>
<contactref element="IC1" pad="30"/>
</signal>
<signal name="D1_TX">
<contactref element="SL3" pad="6"/>
<contactref element="IC1" pad="31"/>
</signal>
<signal name="CE">
<contactref element="RF1" pad="CE"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="CSN">
<contactref element="RF1" pad="CSN"/>
<contactref element="IC1" pad="14"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="IRQ">
<contactref element="RF1" pad="IRQ"/>
<contactref element="IC1" pad="32"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="7"/>
<contactref element="U$3" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="8"/>
<contactref element="U$3" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="R5" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="J1" pad="2"/>
<contactref element="IC1" pad="25"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="24"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="A0">
<contactref element="IC1" pad="23"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="20"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$13">
</signal>
<signal name="N$11">
</signal>
</signals>
</board>
</drawing>
</eagle>
