<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="65.089503125" y1="37" x2="19.01" y2="37.03" width="0" layer="20"/>
<wire x1="19.01" y1="37.03" x2="19.01" y2="35.56" width="0" layer="20"/>
<wire x1="19.01" y1="35.56" x2="10.99" y2="35.56" width="0" layer="20"/>
<wire x1="10.99" y1="35.56" x2="10.947" y2="37" width="0" layer="20"/>
<wire x1="10.947" y1="37" x2="1.910496875" y2="37" width="0" layer="20"/>
<wire x1="1.910496875" y1="37" x2="0" y2="35.089503125" width="0" layer="20"/>
<wire x1="0" y1="35.089503125" x2="0" y2="1.920934375" width="0" layer="20"/>
<wire x1="0" y1="1.920934375" x2="1.920934375" y2="0" width="0" layer="20"/>
<wire x1="1.920934375" y1="0" x2="11.020934375" y2="0" width="0" layer="20"/>
<wire x1="11.020934375" y1="0" x2="11" y2="1.3" width="0" layer="20"/>
<wire x1="11" y1="1.3" x2="20" y2="1.3" width="0" layer="20"/>
<wire x1="20" y1="1.3" x2="20" y2="0" width="0" layer="20"/>
<wire x1="20" y1="0" x2="29.254" y2="0" width="0" layer="20"/>
<wire x1="29.254" y1="0" x2="29.254" y2="-2.4" width="0" layer="20"/>
<wire x1="29.254" y1="-2.4" x2="36" y2="-2.4" width="0" layer="20"/>
<wire x1="36" y1="-2.4" x2="36" y2="0" width="0" layer="20"/>
<wire x1="36" y1="0" x2="47" y2="0" width="0" layer="20"/>
<wire x1="47" y1="0" x2="47" y2="1.3" width="0" layer="20"/>
<wire x1="47" y1="1.3" x2="56" y2="1.3" width="0" layer="20"/>
<wire x1="56" y1="1.3" x2="56" y2="0" width="0" layer="20"/>
<wire x1="56" y1="0" x2="65.089503125" y2="0" width="0" layer="20"/>
<wire x1="65.089503125" y1="0" x2="67" y2="1.910496875" width="0" layer="20"/>
<wire x1="67" y1="1.910496875" x2="67" y2="35.089503125" width="0" layer="20"/>
<wire x1="67" y1="35.089503125" x2="65.089503125" y2="37" width="0" layer="20"/>
<text>MISO VCC
SCK MOSI
RST GND</text>
<text>C_IN</text>
<text>C_RES</text>
<text>3 buttons glass touch
switch replacement board
for MySensors</text>
<text>Replaces LIVOLO VL-C800S-1 / VER : C0 </text>
<text>v0.9 - NCA78 - 10/05/2017</text>
<text>OFF</text>
<text>ON</text>
<text>ON</text>
<text>OFF</text>
<text>ON</text>
<text>OFF</text>
<text>OFF</text>
<text>ON</text>
<text>ON</text>
<text>OFF</text>
<text>ON</text>
<text>OFF</text>
<text>S</text>
<text>T</text>
<text>S</text>
<text>S</text>
<text>T</text>
<text>T</text>
<text>RE2</text>
<text>RE1</text>
<text>LE2</text>
<text>LE3</text>
<text>RELAY 0</text>
<text>RELAY 1</text>
<text>RELAY 2</text>
<text>VCC</text>
<text>GND</text>
<text>R1</text>
<text>10K</text>
<text>100nF</text>
<text>100nF</text>
<text>100nF</text>
<text>10K</text>
<text>RE3</text>
<text>RE4</text>
<text>LE1</text>
<text>LE4</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>VCC MISO
MOSI SCK
GND RST</text>
<hole x="44" y="24" drill="1.5"/>
<hole x="18" y="24" drill="1.5"/>
<hole x="44" y="18" drill="1.5"/>
<text>RX
TX  VCC
RST GND</text>
<text>    RX
VCC TX
GND RST</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206-CAP">
</package>
<package name="EIA3216">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="NCA_Sensors">
<packages>
<package name="CONNECTOR_02_X_07_2MM">
</package>
<package name="TOUCH_PAD_ROUND">
</package>
<package name="SOT-23-6">
</package>
</packages>
</library>
<library name="TD-MySensors">
<packages>
<package name="LED_0805">
<description>&lt;b&gt;0805 Large pad size&lt;/b&gt;&lt;p&gt;

Digikey recommended sizing</description>
</package>
<package name="SOT23-3">
</package>
<package name="DUPONT_3">
</package>
<package name="DUPONT_2">
</package>
<package name="DUPONT_2_3">
</package>
</packages>
</library>
<library name="nrf24l01plus">
<packages>
<package name="WIRELESS-NRF24L01-SMD">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="1206-CAP" value="4.7uF">
<attribute name="PROD_ID" value="CAP-10300"/>
</element>
<element name="C2" library="SparkFun-Passives" package="0805" value="100nF"/>
<element name="C3" library="SparkFun-Passives" package="0805" value="100nF"/>
<element name="C7" library="SparkFun-Passives" package="0805" value="100nF"/>
<element name="CS1" library="SparkFun-Passives" package="0805" value="0-50pF"/>
<element name="CS2" library="SparkFun-Passives" package="0805" value="0-50pF"/>
<element name="CS3" library="SparkFun-Passives" package="0805" value="0-50pF"/>
<element name="CT1" library="SparkFun-Passives" package="0805" value="100nF"/>
<element name="CT2" library="SparkFun-Passives" package="0805" value="100nF"/>
<element name="CT3" library="SparkFun-Passives" package="0805" value="100nF"/>
<element name="J1" library="NCA_Sensors" package="CONNECTOR_02_X_07_2MM" value="CONNECTOR_02_X_072MM_SPACING"/>
<element name="LV1" library="TD-MySensors" package="LED_0805" value=""/>
<element name="LV2" library="TD-MySensors" package="LED_0805" value=""/>
<element name="LV3" library="TD-MySensors" package="LED_0805" value=""/>
<element name="LR3" library="TD-MySensors" package="LED_0805" value=""/>
<element name="LR1" library="TD-MySensors" package="LED_0805" value=""/>
<element name="LR2" library="TD-MySensors" package="LED_0805" value=""/>
<element name="M1" library="nrf24l01plus" package="WIRELESS-NRF24L01-SMD" value="WIRELESS-NRF24L01SMD"/>
<element name="PAD1" library="NCA_Sensors" package="TOUCH_PAD_ROUND" value="TOUCH_PADROUND"/>
<element name="PAD2" library="NCA_Sensors" package="TOUCH_PAD_ROUND" value="TOUCH_PADROUND"/>
<element name="PAD3" library="NCA_Sensors" package="TOUCH_PAD_ROUND" value="TOUCH_PADROUND"/>
<element name="R1" library="SparkFun-Passives" package="0805" value="10k"/>
<element name="R2" library="SparkFun-Passives" package="0805" value="10K"/>
<element name="TTP1" library="NCA_Sensors" package="SOT-23-6" value="TTP223-BA6"/>
<element name="TTP2" library="NCA_Sensors" package="SOT-23-6" value="TTP223-BA6"/>
<element name="TTP3" library="NCA_Sensors" package="SOT-23-6" value="TTP223-BA6"/>
<element name="U1" library="SparkFun-DigitalIC" package="TQFP32-08" value="ATMEGA328P_TQFP">
<attribute name="PROD_ID" value="IC-09069"/>
</element>
<element name="U2" library="TD-MySensors" package="SOT23-3" value=""/>
<element name="U$2" library="TD-MySensors" package="DUPONT_3" value=""/>
<element name="U$3" library="TD-MySensors" package="DUPONT_2" value=""/>
<element name="C_RES" library="SparkFun-Capacitors" package="EIA3216" value="100uF">
<attribute name="PROD_ID" value="CAP-00811"/>
</element>
<element name="C_IN" library="SparkFun-Capacitors" package="EIA3216" value="4.7uF">
<attribute name="PROD_ID" value="CAP-00811"/>
</element>
<element name="RV1" library="SparkFun-Passives" package="0805" value=""/>
<element name="RR1" library="SparkFun-Passives" package="0805" value=""/>
<element name="RV2" library="SparkFun-Passives" package="0805" value=""/>
<element name="RR2" library="SparkFun-Passives" package="0805" value=""/>
<element name="RV3" library="SparkFun-Passives" package="0805" value=""/>
<element name="RR3" library="SparkFun-Passives" package="0805" value=""/>
<element name="RE1" library="SparkFun-Passives" package="0805" value=""/>
<element name="RE2" library="SparkFun-Passives" package="0805" value=""/>
<element name="LE1" library="TD-MySensors" package="LED_0805" value=""/>
<element name="LE2" library="TD-MySensors" package="LED_0805" value=""/>
<element name="C_4" library="SparkFun-Capacitors" package="EIA3216" value="10uF">
<attribute name="PROD_ID" value="CAP-00811"/>
</element>
<element name="J2" library="TD-MySensors" package="DUPONT_2_3" value=""/>
<element name="LE3" library="TD-MySensors" package="LED_0805" value=""/>
<element name="LE4" library="TD-MySensors" package="LED_0805" value=""/>
<element name="RE3" library="SparkFun-Passives" package="0805" value=""/>
<element name="RE4" library="SparkFun-Passives" package="0805" value=""/>
</elements>
<signals>
<signal name="RESET">
<contactref element="U1" pad="29"/>
<contactref element="R1" pad="2"/>
<contactref element="U$2" pad="3"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="VCC">
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="6"/>
<contactref element="M1" pad="8"/>
<contactref element="C1" pad="1"/>
<contactref element="U2" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="TTP1" pad="5"/>
<contactref element="CT1" pad="1"/>
<contactref element="TTP3" pad="5"/>
<contactref element="CT3" pad="1"/>
<contactref element="TTP2" pad="5"/>
<contactref element="CT2" pad="1"/>
<contactref element="LV2" pad="1"/>
<contactref element="J1" pad="10"/>
<contactref element="U$3" pad="1"/>
<contactref element="C_IN" pad="A"/>
<contactref element="C_RES" pad="A"/>
<contactref element="U1" pad="18"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="20"/>
<contactref element="RV1" pad="1"/>
<contactref element="RV3" pad="1"/>
<contactref element="C_4" pad="A"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="GND">
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="21"/>
<contactref element="C1" pad="2"/>
<contactref element="M1" pad="7"/>
<contactref element="U2" pad="3"/>
<contactref element="C7" pad="1"/>
<contactref element="CS3" pad="2"/>
<contactref element="TTP3" pad="2"/>
<contactref element="CT3" pad="2"/>
<contactref element="J1" pad="8"/>
<contactref element="CS1" pad="2"/>
<contactref element="TTP1" pad="2"/>
<contactref element="CT1" pad="2"/>
<contactref element="CS2" pad="2"/>
<contactref element="TTP2" pad="2"/>
<contactref element="CT2" pad="2"/>
<contactref element="U$3" pad="2"/>
<contactref element="C_RES" pad="C"/>
<contactref element="C_IN" pad="C"/>
<contactref element="RR1" pad="2"/>
<contactref element="LR2" pad="2"/>
<contactref element="RR3" pad="2"/>
<contactref element="RE1" pad="2"/>
<contactref element="RE2" pad="2"/>
<contactref element="C_4" pad="C"/>
<contactref element="J2" pad="1"/>
<contactref element="RE4" pad="2"/>
</signal>
<signal name="CE">
<contactref element="M1" pad="6"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="CSN">
<contactref element="M1" pad="5"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="SCK">
<contactref element="M1" pad="4"/>
<contactref element="U1" pad="17"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="MOSI">
<contactref element="M1" pad="3"/>
<contactref element="U1" pad="15"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="M1" pad="2"/>
<contactref element="U1" pad="16"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="IRQ_NRF">
<contactref element="U1" pad="32"/>
</signal>
<signal name="A3_ATSHA">
<contactref element="U2" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="26"/>
</signal>
<signal name="TOUCH_1">
<contactref element="TTP1" pad="1"/>
<contactref element="U1" pad="22"/>
</signal>
<signal name="TOUCH_2">
<contactref element="TTP2" pad="1"/>
<contactref element="U1" pad="25"/>
</signal>
<signal name="TOUCH_3">
<contactref element="U1" pad="19"/>
<contactref element="TTP3" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="TTP1" pad="3"/>
<contactref element="CS1" pad="1"/>
<contactref element="PAD1" pad="SENSEPAD"/>
</signal>
<signal name="N$4">
<contactref element="TTP2" pad="3"/>
<contactref element="CS2" pad="1"/>
<contactref element="PAD2" pad="SENSEPAD"/>
</signal>
<signal name="N$5">
<contactref element="TTP3" pad="3"/>
<contactref element="CS3" pad="1"/>
<contactref element="PAD3" pad="SENSEPAD"/>
</signal>
<signal name="LED1">
<contactref element="U1" pad="9"/>
<contactref element="LV1" pad="2"/>
<contactref element="LR1" pad="1"/>
</signal>
<signal name="LED2">
<contactref element="U1" pad="10"/>
<contactref element="RV2" pad="2"/>
<contactref element="RR2" pad="1"/>
</signal>
<signal name="LED3">
<contactref element="U1" pad="12"/>
<contactref element="LV3" pad="2"/>
<contactref element="LR3" pad="1"/>
</signal>
<signal name="RX">
<contactref element="U1" pad="30"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="TX">
<contactref element="U1" pad="31"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="RELAY0">
<contactref element="J1" pad="5"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="RELAY1">
<contactref element="U1" pad="2"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="RELAY2">
<contactref element="J1" pad="1"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="N$1">
<contactref element="RV1" pad="2"/>
<contactref element="LV1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="LR1" pad="2"/>
<contactref element="RR1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="RV2" pad="1"/>
<contactref element="LV2" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="RR2" pad="2"/>
<contactref element="LR2" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="RV3" pad="2"/>
<contactref element="LV3" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="LR3" pad="2"/>
<contactref element="RR3" pad="1"/>
</signal>
<signal name="LED_EX1">
<contactref element="LE1" pad="1"/>
<contactref element="U1" pad="23"/>
</signal>
<signal name="LED_EX2">
<contactref element="U1" pad="28"/>
<contactref element="LE2" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="RE1" pad="1"/>
<contactref element="LE1" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="RE2" pad="1"/>
<contactref element="LE2" pad="2"/>
</signal>
<signal name="LED_EX3">
<contactref element="LE3" pad="1"/>
<contactref element="U1" pad="27"/>
</signal>
<signal name="LED_EX4">
<contactref element="U1" pad="24"/>
<contactref element="LE4" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="LE3" pad="2"/>
<contactref element="RE3" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="LE4" pad="2"/>
<contactref element="RE4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
