<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="48.26" y2="0" width="0" layer="20"/>
<wire x1="48.26" y1="0" x2="48.26" y2="23" width="0" layer="20"/>
<wire x1="48.26" y1="23" x2="0" y2="23" width="0" layer="20"/>
<wire x1="0" y1="23" x2="0" y2="0" width="0" layer="20"/>
<text>RAW</text>
<text>GND</text>
<text>VCC</text>
<text>SCL</text>
<text>SDA</text>
<text>MI LIGHT SHIELD 
FOR NMODULE
v0.1 - NCA78
18/05/2017</text>
<text>C1 10uF</text>
<hole x="46.6" y="21.5" drill="2"/>
<text>GREEN</text>
<text>RED</text>
<text>-</text>
<text>+</text>
<hole x="26" y="1.5" drill="2"/>
<hole x="1.5" y="21.5" drill="2"/>
<text>C2 10uF</text>
<text>AMS1117</text>
<text>3.3V FROM NMODULE</text>
<text>SHORT HERE TO USE</text>
<text>C5 100nF</text>
<text>C6</text>
<text>C3 - 100nF
(AMS1117 OUTPUT)</text>
<text>A</text>
<text>3</text>
<text>4</text>
<text>2</text>
<text>1</text>
<text>4</text>
<text>3</text>
<text>2</text>
<text>1</text>
<text>B</text>
</plain>
<libraries>
<library name="TD-MySensors">
<packages>
<package name="DUPONT_10">
</package>
<package name="DUPONT_5">
</package>
<package name="DUPONT_4">
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="PAD-JUMPER-2-NO_YES_SILK">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
<package name="CAP_0805">
<description>&lt;b&gt;0805 Large pad size&lt;/b&gt;&lt;p&gt;

Digikey recommended sizing</description>
</package>
<package name="R_0805">
<description>&lt;b&gt;0805 Large pad size&lt;/b&gt;&lt;p&gt;

Digikey recommended sizing</description>
</package>
</packages>
</library>
<library name="User-Submitted">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find submitted parts from SparkFun users everywhere!&lt;br&gt;&lt;br&gt;
These are not necessarily parts we carry, but are parts that other users have determined function well with other parts in our libraries. Please keep in mind that it is the end user's responsibility to ensure correctness and suitablity for a given componet or application.
&lt;br&gt;&lt;br&gt;
If you find these parts useful, please consider helping the open-source community by contributing your own through GitHub. https://github.com/sparkfun/SparkFun-Eagle-Libraries
&lt;br&gt;&lt;br&gt;

&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-DUALCOLOR-3MM">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="CPOL-RADIAL-10UF-25V">
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-MINIB">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="WS2812B">
<description>&lt;b&gt;Intelligent control LED with integrated light source&lt;/b&gt;&lt;p&gt;
WS2812B&lt;br&gt;
source: http://www.world-semi.com/uploads/soft/130904/1_1500205981.pdf</description>
</package>
</packages>
</library>
<library name="nrf24l01plus">
<packages>
<package name="WIRELESS-NRF24L01-SMD">
</package>
</packages>
</library>
<library name="NCA_Sensors">
<packages>
<package name="SWITCH_SMD_PROMINI_RESET">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="NMODULE" library="TD-MySensors" package="DUPONT_10" value="CONNECTOR_10DUPONT"/>
<element name="SPI_PROMINI" library="TD-MySensors" package="DUPONT_4" value=""/>
<element name="PINS4_9_PROMINI" library="TD-MySensors" package="DUPONT_5" value=""/>
<element name="U$5" library="User-Submitted" package="LED-DUALCOLOR-3MM" value="LED-DUALCOLOR3MM-THROUGH-HOLE"/>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.4" value=""/>
<element name="J1" library="SparkFun-Connectors" package="USB-MINIB" value="USBSMD">
<attribute name="PROD_ID" value="CONN-08193"/>
</element>
<element name="D1" library="SparkFun-LED" package="WS2812B" value="">
<attribute name="PROD_ID" value="DIO-12503"/>
</element>
<element name="M1" library="nrf24l01plus" package="WIRELESS-NRF24L01-SMD" value="WIRELESS-NRF24L01SMD"/>
<element name="U1" library="TD-MySensors" package="SOT223" value=""/>
<element name="JREG2" library="TD-MySensors" package="PAD-JUMPER-2-NO_YES_SILK" value=""/>
<element name="C1" library="SparkFun-Passives" package="CPOL-RADIAL-10UF-25V" value="10uF"/>
<element name="C2" library="TD-MySensors" package="CAP_0805" value="10uF"/>
<element name="C3" library="SparkFun-Passives" package="0805" value="100nF"/>
<element name="C5" library="SparkFun-Passives" package="0805" value="100nF"/>
<element name="C6" library="SparkFun-Passives" package="0805" value=""/>
<element name="D3" library="SparkFun-LED" package="WS2812B" value="">
<attribute name="PROD_ID" value="DIO-12503"/>
</element>
<element name="D2" library="SparkFun-LED" package="WS2812B" value="">
<attribute name="PROD_ID" value="DIO-12503"/>
</element>
<element name="D4" library="SparkFun-LED" package="WS2812B" value="">
<attribute name="PROD_ID" value="DIO-12503"/>
</element>
<element name="R2" library="TD-MySensors" package="R_0805" value="150"/>
<element name="R3" library="TD-MySensors" package="R_0805" value="150"/>
<element name="R4" library="TD-MySensors" package="R_0805" value="150"/>
<element name="R5" library="TD-MySensors" package="R_0805" value="150"/>
<element name="C10" library="TD-MySensors" package="CAP_0805" value="100nF"/>
<element name="C4" library="TD-MySensors" package="CAP_0805" value="100nF"/>
<element name="C8" library="TD-MySensors" package="CAP_0805" value="100nF"/>
<element name="C9" library="TD-MySensors" package="CAP_0805" value="100nF"/>
<element name="BT1" library="NCA_Sensors" package="SWITCH_SMD_PROMINI_RESET" value="SWITCHPROMINI_RESET"/>
<element name="BT2" library="NCA_Sensors" package="SWITCH_SMD_PROMINI_RESET" value="SWITCHPROMINI_RESET"/>
<element name="BT3" library="NCA_Sensors" package="SWITCH_SMD_PROMINI_RESET" value="SWITCHPROMINI_RESET"/>
<element name="BT4" library="NCA_Sensors" package="SWITCH_SMD_PROMINI_RESET" value="SWITCHPROMINI_RESET"/>
<element name="BT5" library="NCA_Sensors" package="SWITCH_SMD_PROMINI_RESET" value="SWITCHPROMINI_RESET"/>
<element name="BT6" library="NCA_Sensors" package="SWITCH_SMD_PROMINI_RESET" value="SWITCHPROMINI_RESET"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="NMODULE" pad="3"/>
<contactref element="U1" pad="2" route="any" routetag="G$1.VOUT@1"/>
<contactref element="U1" pad="4" route="any" routetag="G$1.VOUT@1"/>
<contactref element="M1" pad="8"/>
<contactref element="JREG2" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="GND">
<contactref element="NMODULE" pad="2"/>
<contactref element="R1" pad="P$1"/>
<contactref element="J1" pad="GND"/>
<contactref element="M1" pad="7"/>
<contactref element="U1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="D2" pad="3"/>
<contactref element="D3" pad="3"/>
<contactref element="D1" pad="3"/>
<contactref element="D4" pad="3"/>
<contactref element="C10" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="BT1" pad="OUT"/>
<contactref element="BT2" pad="OUT"/>
<contactref element="BT3" pad="OUT"/>
<contactref element="BT4" pad="OUT"/>
<contactref element="BT5" pad="OUT"/>
<contactref element="BT6" pad="OUT"/>
</signal>
<signal name="RAW">
<contactref element="NMODULE" pad="1"/>
<contactref element="J1" pad="VBUS"/>
<contactref element="U1" pad="3"/>
<contactref element="JREG2" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="A4_SDA">
<contactref element="NMODULE" pad="5"/>
<contactref element="BT5" pad="IN"/>
</signal>
<signal name="D3">
<contactref element="NMODULE" pad="7"/>
<contactref element="BT2" pad="IN"/>
</signal>
<signal name="A3">
<contactref element="NMODULE" pad="8"/>
</signal>
<signal name="A2">
<contactref element="NMODULE" pad="9"/>
<contactref element="U$5" pad="A2"/>
</signal>
<signal name="A1">
<contactref element="NMODULE" pad="10"/>
<contactref element="U$5" pad="A1"/>
<contactref element="D1" pad="4"/>
</signal>
<signal name="D2">
<contactref element="NMODULE" pad="6"/>
<contactref element="BT1" pad="IN"/>
</signal>
<signal name="A5_SCL">
<contactref element="NMODULE" pad="4"/>
<contactref element="BT6" pad="IN"/>
</signal>
<signal name="MOSI">
<contactref element="SPI_PROMINI" pad="2"/>
<contactref element="M1" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="SPI_PROMINI" pad="3"/>
<contactref element="M1" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="SPI_PROMINI" pad="4"/>
<contactref element="M1" pad="4"/>
</signal>
<signal name="CSN">
<contactref element="M1" pad="5"/>
<contactref element="PINS4_9_PROMINI" pad="2"/>
</signal>
<signal name="CE">
<contactref element="M1" pad="6"/>
<contactref element="PINS4_9_PROMINI" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="U$5" pad="K"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="N$3">
<contactref element="D1" pad="2"/>
<contactref element="D3" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="D3" pad="2"/>
<contactref element="D2" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="D2" pad="2"/>
<contactref element="D4" pad="4"/>
</signal>
<signal name="N$7">
<contactref element="R5" pad="1"/>
<contactref element="D4" pad="1"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R4" pad="1"/>
<contactref element="D2" pad="1"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R3" pad="1"/>
<contactref element="D3" pad="1"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R2" pad="1"/>
<contactref element="D1" pad="1"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="D6">
<contactref element="PINS4_9_PROMINI" pad="4"/>
<contactref element="BT4" pad="IN"/>
</signal>
<signal name="D5">
<contactref element="PINS4_9_PROMINI" pad="5"/>
<contactref element="BT3" pad="IN"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
