<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0.127" y1="35.814" x2="3.302" y2="43.434" width="0" layer="20"/>
<wire x1="3.302" y1="43.434" x2="45.466" y2="43.434" width="0" layer="20"/>
<wire x1="45.466" y1="43.434" x2="48.641" y2="35.814" width="0" layer="20"/>
<wire x1="48.641" y1="35.814" x2="48.641" y2="0" width="0" layer="20"/>
<wire x1="48.641" y1="0" x2="0.127" y2="0" width="0" layer="20"/>
<wire x1="0.127" y1="0" x2="0.127" y2="35.814" width="0" layer="20"/>
<wire x1="9.417" y1="3.148" x2="9.544" y2="21.436" width="1.6764" layer="46"/>
<wire x1="15.186" y1="3.248" x2="15.2" y2="8.9" width="1.6764" layer="46"/>
<wire x1="15.2" y1="8.9" x2="15.886" y2="16.38" width="1.6764" layer="46"/>
<wire x1="15.886" y1="16.38" x2="17.364" y2="17.707" width="1.6764" layer="46"/>
<wire x1="17.364" y1="17.707" x2="21.844" y2="21.463" width="1.6764" layer="46"/>
<wire x1="21.844" y1="21.463" x2="26.67" y2="22.987" width="1.6764" layer="46"/>
<wire x1="26.67" y1="22.987" x2="36.414" y2="26.154" width="1.6764" layer="46"/>
<wire x1="36.414" y1="26.154" x2="36.214" y2="31.823" width="1.9304" layer="46"/>
<wire x1="36.214" y1="31.823" x2="31.796" y2="31.796" width="1.9304" layer="46"/>
<wire x1="19.431" y1="7.366" x2="19.812" y2="8.509" width="1.6764" layer="46"/>
<wire x1="19.812" y1="8.509" x2="21.717" y2="13.081" width="1.6764" layer="46"/>
<wire x1="44.45" y1="14.351" x2="38.9" y2="14.1" width="1.6764" layer="46"/>
<wire x1="38.9" y1="14.1" x2="35.941" y2="13.435" width="1.6764" layer="46"/>
<wire x1="35.941" y1="13.435" x2="36.268" y2="8.644" width="1.6764" layer="46"/>
<wire x1="36.268" y1="8.644" x2="31.775" y2="7.909" width="1.6764" layer="46"/>
<hole x="8" y="41" drill="2.5"/>
<hole x="44" y="41" drill="2.5"/>
<text>VCC
SCL
SDA
GND</text>
<wire x1="24.13" y1="13.589" x2="21.717" y2="13.081" width="1.6764" layer="46"/>
<text>IN - NEUTRAL</text>
<text>IN - PHASE</text>
<text>OUT - NEUTRAL</text>
<text>OUT - NEUTRAL</text>
<text>OUT - PHASE 1</text>
<text>OUT - PHASE 2</text>
<wire x1="42.291" y1="2.54" x2="41.275" y2="11.43" width="1.6764" layer="46"/>
<wire x1="9.5" y1="21.4" x2="19.431" y2="28.067" width="1.6764" layer="46"/>
<wire x1="19.431" y1="28.067" x2="26.675" y2="29.829" width="1.6764" layer="46"/>
<wire x1="36.549" y1="2.159" x2="35.787" y2="5.588" width="1.6764" layer="46"/>
<wire x1="29.743" y1="18.376" x2="32.385" y2="18.161" width="1.6764" layer="46"/>
<wire x1="32.385" y1="18.161" x2="38.692" y2="21.078" width="1.6764" layer="46"/>
<text>Light / 2SSR shield 
for NModule
NCA78 - v0.2
15/05/2017</text>
<text>/!\ WARNING HIGH VOLTAGE /!\</text>
<text>/!\ WARNING HIGH VOLTAGE /!\</text>
</plain>
<libraries>
<library name="TD-MySensors">
<packages>
<package name="HKLPM01">
</package>
<package name="RELAY_G3MB_SPST">
<description>G3MB Relay</description>
</package>
<package name="DUPONT_4">
</package>
</packages>
</library>
<library name="NCA_Sensors">
<packages>
<package name="FUSE_AXIAL_VERTICAL">
</package>
<package name="SCREW_CONNECTOR_2X">
</package>
<package name="VARISTOR">
</package>
<package name="NMODULE_VERTICAL">
</package>
</packages>
</library>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-92-AMMO">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-10UF-25V">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1/6W-RES">
<description>1/6W Thru-hole Resistor - *UNPROVEN*</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="HKLP1" library="TD-MySensors" package="HKLPM01" value="HKLPM01"/>
<element name="K1" library="TD-MySensors" package="RELAY_G3MB_SPST" value="SSR"/>
<element name="INPUT_FUSE" library="NCA_Sensors" package="FUSE_AXIAL_VERTICAL" value="FUSEAXIAL_11_36_VERTICAL"/>
<element name="OUT_NEUTRAL" library="NCA_Sensors" package="SCREW_CONNECTOR_2X" value="SCREW_CONNECTOR_2X"/>
<element name="VARISTOR" library="NCA_Sensors" package="VARISTOR" value="VARISTOR"/>
<element name="IN" library="NCA_Sensors" package="SCREW_CONNECTOR_2X" value="SCREW_CONNECTOR_2X"/>
<element name="J_I2C" library="TD-MySensors" package="DUPONT_4" value=""/>
<element name="DS18" library="SparkFun-Sensors" package="TO-92-AMMO" value="DS18B20">
<attribute name="STORE_ID" value="SEN-00245"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value=""/>
<element name="U$3" library="NCA_Sensors" package="NMODULE_VERTICAL" value="NMODULEVERTICAL"/>
<element name="K2" library="TD-MySensors" package="RELAY_G3MB_SPST" value="SSR"/>
<element name="OUT_PHASE" library="NCA_Sensors" package="SCREW_CONNECTOR_2X" value="SCREW_CONNECTOR_2X"/>
<element name="C2" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value=""/>
<element name="R1" library="SparkFun-Passives" package="1/6W-RES" value="4.7K"/>
<element name="TEMP_FUSE" library="NCA_Sensors" package="FUSE_AXIAL_VERTICAL" value="FUSEAXIAL_11_36_VERTICAL"/>
</elements>
<signals>
<signal name="GND">
<contactref element="HKLP1" pad="P$3"/>
<contactref element="K1" pad="4"/>
<contactref element="DS18" pad="1"/>
<contactref element="U$3" pad="GND"/>
<contactref element="K2" pad="4"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="J_I2C" pad="1"/>
</signal>
<signal name="IN_PHASE">
<contactref element="IN" pad="P$1"/>
<contactref element="INPUT_FUSE" pad="P$2"/>
</signal>
<signal name="VCC">
<contactref element="DS18" pad="3"/>
<contactref element="U$3" pad="VCC"/>
<contactref element="J_I2C" pad="4"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="IN_NEUTRAL">
<contactref element="HKLP1" pad="P$2"/>
<contactref element="OUT_NEUTRAL" pad="P$1"/>
<contactref element="IN" pad="P$2"/>
<contactref element="VARISTOR" pad="P$1"/>
<contactref element="OUT_NEUTRAL" pad="P$2"/>
</signal>
<signal name="OUT_PHASE">
<contactref element="K1" pad="1"/>
<contactref element="OUT_PHASE" pad="P$1"/>
</signal>
<signal name="IN_FUSED">
<contactref element="HKLP1" pad="P$1"/>
<contactref element="K1" pad="2"/>
<contactref element="VARISTOR" pad="P$2"/>
<contactref element="K2" pad="2"/>
<contactref element="TEMP_FUSE" pad="P$2"/>
</signal>
<signal name="SCL">
<contactref element="U$3" pad="SCL"/>
<contactref element="J_I2C" pad="3"/>
</signal>
<signal name="SDA">
<contactref element="U$3" pad="SDA"/>
<contactref element="J_I2C" pad="2"/>
</signal>
<signal name="DS18DQ">
<contactref element="DS18" pad="2"/>
<contactref element="U$3" pad="D3"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="RAW">
<contactref element="HKLP1" pad="P$4"/>
<contactref element="U$3" pad="RAW"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="OUT_PHASE1">
<contactref element="K2" pad="1"/>
<contactref element="OUT_PHASE" pad="P$2"/>
</signal>
<signal name="SSR_TRIGGER1">
<contactref element="K1" pad="3"/>
<contactref element="U$3" pad="A2"/>
</signal>
<signal name="SSR_TRIGGER2">
<contactref element="K2" pad="3"/>
<contactref element="U$3" pad="A1"/>
</signal>
<signal name="N$1">
<contactref element="INPUT_FUSE" pad="P$1"/>
<contactref element="TEMP_FUSE" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
