<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="10.16" y2="0" width="0" layer="20"/>
<wire x1="10.16" y1="0" x2="10.16" y2="12.69" width="0" layer="20"/>
<wire x1="10.16" y1="12.69" x2="0" y2="12.69" width="0" layer="20"/>
<wire x1="0" y1="12.69" x2="0" y2="0" width="0" layer="20"/>
<text>ICSP PogoPin adapter</text>
<text>2017, Public Domain</text>
</plain>
<libraries>
<library name="analyzer">
<packages>
<package name="2X03">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="analyzer" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="J5" library="analyzer" package="2X03" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="MOSI">
<contactref element="J5" pad="4"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="J5" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="J5" pad="3"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="J5" pad="6"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="VCC_5V">
<contactref element="J5" pad="2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="J5" pad="5"/>
<contactref element="J1" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
