<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0.0254" y1="0" x2="19.3094" y2="0" width="0" layer="20"/>
<wire x1="19.3094" y1="0" x2="19.3094" y2="14.5288" width="0" layer="20"/>
<wire x1="19.3094" y1="14.5288" x2="0.0254" y2="14.5288" width="0" layer="20"/>
<wire x1="0.0254" y1="14.5288" x2="0.0254" y2="0" width="0" layer="20"/>
<text>A3</text>
<text>MOSI</text>
<text>SCK</text>
<text>MISO</text>
<text>D8</text>
<text>GND</text>
<text>3V</text>
</plain>
<libraries>
<library name="Sensor_tbowmo">
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="microchip">
<description>&lt;b&gt;Microchip PIC Microcontrollers and other Devices&lt;/b&gt;&lt;p&gt;
Based on the following sources :
&lt;ul&gt;
&lt;li&gt;Microchip Data Book, 1993
&lt;li&gt;THE EMERGING WORLD STANDARD, 1995/1996
&lt;li&gt;Microchip, Technical Library CD-ROM, June 1998
&lt;li&gt;www.microchip.com
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO-08">
<description>&lt;B&gt;Small Outline Narrow Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
150-mil body, package type SN</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X07">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="LowPowerLab">
<packages>
<package name="1206">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ATSHA" library="Sensor_tbowmo" package="SOT23" value="ATSHA204A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="EEPROM" library="microchip" package="SO-08" value="AT25DF512C-SSHN-B">
<attribute name="OC_NEWARK" value="92C7351"/>
<attribute name="MPN" value="25AA080/SN"/>
<attribute name="MF" value="MICROCHIP"/>
<attribute name="OC_FARNELL" value="1816072"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinhead" package="1X07" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="1206" value="56k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="LowPowerLab" package="1206" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="LowPowerLab" package="1206" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="1206" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="ATSHA" pad="2"/>
<contactref element="EEPROM" pad="7"/>
<contactref element="EEPROM" pad="3"/>
<contactref element="EEPROM" pad="8"/>
<contactref element="R1" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="ATSHA" pad="3"/>
<contactref element="EEPROM" pad="4"/>
<contactref element="JP2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="EEPROM" pad="6"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="MISO">
<contactref element="EEPROM" pad="2"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="MOSI">
<contactref element="EEPROM" pad="5"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="A3">
<contactref element="ATSHA" pad="1"/>
<contactref element="JP2" pad="7"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="D8">
<contactref element="EEPROM" pad="1"/>
<contactref element="JP2" pad="3"/>
<contactref element="R1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
