<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<text>V2</text>
<hole x="11.6332" y="49.0982" drill="3.0638"/>
<hole x="44.6532" y="49.0982" drill="3.0638"/>
<text>Config</text>
<wire x1="54.0512" y1="39.6748" x2="53.8734" y2="21.1074" width="0.127" layer="20" curve="-180"/>
<wire x1="54.0258" y1="39.6494" x2="2.0574" y2="21.3614" width="0.127" layer="20" curve="180"/>
<wire x1="53.7972" y1="21.0312" x2="2.413" y2="40.8178" width="0.127" layer="20" curve="-182.090905"/>
<text>PUT NODEMCU
    HERE</text>
<text>USB</text>
<text>Happy Bubbles
  Technology</text>
<text>HAPPY BUBBLES
TECHNOLOGY</text>
<text> V2
2016</text>
<text>www.happybubbles.tech</text>
</plain>
<libraries>
<library name="lio">
<packages>
<package name="PTR5518">
</package>
</packages>
</library>
<library name="ESP12E_DEVKIT">
<packages>
<package name="ESP12E_DEVKIT">
<description>ESP12E_DEVKIT</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
<package name="OSHW-LOGO-L">
</package>
</packages>
</library>
<library name="tag-connect">
<description>&lt;h3&gt;TAG-CONNECT ICSP Connector&lt;/h3&gt;&lt;BR&gt;&lt;I&gt;Manufacturer:&lt;/I&gt; &lt;a href="http://www.tag-connect.com"&gt;Tag-Connect&lt;/a&gt;&lt;BR&gt;
&lt;BR&gt;Cable for easy In-Circuit Serial Programming. Designed for Microchip ICD2, suitable for many others.&lt;BR&gt;
Two variants - one "with legs" (for hands-free fit on PCB) and another "without legs" for quick programming.

&lt;p&gt;
&lt;TABLE cellspacing=0 cellpadding=0 border=0&gt;
&lt;TR&gt;&lt;TD width=20&gt;&lt;/TD&gt;&lt;TD&gt;
&lt;TABLE cellspacing=0 cellpadding=1 border=1&gt;
&lt;TR bgcolor=silver&gt;&lt;TD align=center&gt;PAD&lt;/TD&gt;&lt;TD align=center&gt;Description&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;1&lt;/TD&gt;&lt;TD&gt;MCLR/Vpp&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;2&lt;/TD&gt;&lt;TD&gt;Vdd&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;3&lt;/TD&gt;&lt;TD&gt;GND&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;4&lt;/TD&gt;&lt;TD&gt;PGD (ISPDAT)&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;5&lt;/TD&gt;&lt;TD&gt;PGC (ISPCLK)&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;6&lt;/TD&gt;&lt;TD&gt;nc (used for LVP)&lt;/TD&gt;&lt;/TR&gt;
&lt;/TABLE&gt;
&lt;/TD&gt;&lt;/TR&gt;&lt;/TABLE&gt;&lt;BR&gt;&lt;BR&gt;

©2009 ROFA.cz - modified and updated by Robert Darlington &amp;#8249;rdarlington@gmail.com&amp;#8250;</description>
<packages>
<package name="TC2030-MCP-NL">
<description>&lt;B&gt;TAG-CONNECT ICSP Connector&lt;/B&gt;&lt;BR&gt;&lt;I&gt;Manufacturer:&lt;/I&gt; &lt;a href="www.tag-connect.com"&gt;Tag-Connect&lt;/a&gt;&lt;BR&gt;
&lt;BR&gt;Cable for easy In-Circuit Serial Programming. Designed for Microchip ICD2, suitable for many others.&lt;BR&gt;

&lt;TABLE cellspacing=0 cellpadding=0 border=0&gt;
&lt;TR&gt;&lt;TD width=20&gt;&lt;/TD&gt;&lt;TD&gt;
&lt;TABLE cellspacing=0 cellpadding=1 border=1&gt;
&lt;TR bgcolor=silver&gt;&lt;TD align=center&gt;PAD&lt;/TD&gt;&lt;TD align=center&gt;Description&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;1&lt;/TD&gt;&lt;TD&gt;MCLR/Vpp&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;2&lt;/TD&gt;&lt;TD&gt;Vdd&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;3&lt;/TD&gt;&lt;TD&gt;GND&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;4&lt;/TD&gt;&lt;TD&gt;PGD (ISPDAT)&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;5&lt;/TD&gt;&lt;TD&gt;PGC (ISPCLK)&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;6&lt;/TD&gt;&lt;TD&gt;nc (used for LVP)&lt;/TD&gt;&lt;/TR&gt;
&lt;/TABLE&gt;
&lt;/TD&gt;&lt;/TR&gt;&lt;/TABLE&gt;&lt;BR&gt;&lt;BR&gt;

©2009 ROFA.cz - modified and updated by Robert Darlington &amp;#8249;rdarlington@gmail.com&amp;#8250;</description>
</package>
</packages>
</library>
<library name="CEDT">
<description>&lt;b&gt;Center for Electronics Design and Technology&lt;/b&gt;&lt;br&gt;
at&lt;br&gt;
Netaji Subhas Institute of Technology&lt;br&gt;
Dwarka,&lt;br&gt;
New Delhi, India&lt;br&gt;
&lt;br&gt;
Data Modified : 20-January-2012&lt;br&gt;
&lt;br&gt;
CEDT is Managed by Dhananjay V. Gadre (dvgadre@gmail.com)&lt;br&gt;&lt;br&gt;
&lt;author&gt;This library was created by Anurag Chugh, Rohit Dureja and Shanjit Singh Jajmann&lt;/author&gt;</description>
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SnapButton">
<packages>
<package name="HAPPY_HIPPO">
</package>
<package name="HAPPY_HIPPO_500MIL">
</package>
</packages>
</library>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="C603">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-SWITCH-1101NE">
<description>SparkFun SKU# COM-08229</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="WS2812B">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="lio" package="PTR5518" value="PTR5518"/>
<element name="U2" library="ESP12E_DEVKIT" package="ESP12E_DEVKIT" value="ESP12E_DEVKIT"/>
<element name="C1" library="SparkFun" package="0603-CAP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="tag-connect" package="TC2030-MCP-NL" value=""/>
<element name="C2" library="dp_devices" package="C603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun-Electromechanical" package="TACTILE-SWITCH-1101NE" value="SWITCH-MOMENTARY-2SMD-1101NE">
<attribute name="PROD_ID" value="SWCH-00815"/>
</element>
<element name="R1" library="CEDT" package="R0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="U$5" library="SnapButton" package="HAPPY_HIPPO" value=""/>
<element name="U$1" library="SnapButton" package="HAPPY_HIPPO_500MIL" value=""/>
<element name="L1" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="R2" library="CEDT" package="R0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="U$4" library="SparkFun" package="OSHW-LOGO-L" value=""/>
<element name="U$6" library="SparkFun" package="OSHW-LOGO-L" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="U2" pad="GND@0"/>
<contactref element="U2" pad="GND@1"/>
<contactref element="C2" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="P$9"/>
<contactref element="U1" pad="P$8"/>
<contactref element="J1" pad="3"/>
<contactref element="L1" pad="3-GND"/>
<contactref element="U2" pad="GND@3"/>
<contactref element="U2" pad="GND@2"/>
</signal>
<signal name="3V3">
<contactref element="U2" pad="3V3@1"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="P$10"/>
<contactref element="J1" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="SWCLK">
<contactref element="U1" pad="P$5"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="SWDIO">
<contactref element="U1" pad="P$4"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="BT_TX">
<contactref element="U1" pad="P$2"/>
<contactref element="U2" pad="RX"/>
</signal>
<signal name="WS_LED">
<contactref element="U2" pad="D2"/>
<contactref element="L1" pad="4-DIN"/>
</signal>
<signal name="5V_VIN">
<contactref element="U2" pad="VIN"/>
<contactref element="C2" pad="1"/>
<contactref element="L1" pad="1-VDD"/>
</signal>
<signal name="BTN">
<contactref element="S1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="U2" pad="D6"/>
</signal>
<signal name="3V3_1">
<contactref element="R1" pad="2"/>
<contactref element="U2" pad="3V3@0"/>
</signal>
<signal name="BT_RX">
<contactref element="U1" pad="P$1"/>
<contactref element="U2" pad="TX"/>
</signal>
<signal name="VDD">
<contactref element="J1" pad="2"/>
</signal>
<signal name="BT_ENABLE">
<contactref element="U2" pad="D1"/>
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="P$12"/>
</signal>
<signal name="ESP_RESET">
<contactref element="U1" pad="P$15"/>
<contactref element="U2" pad="RST"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
