<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="29.261" y2="0" width="0.4064" layer="20"/>
<wire x1="29.261" y1="0" x2="29.261" y2="29.2" width="0.4064" layer="20"/>
<wire x1="29.261" y1="29.2" x2="0" y2="29.2" width="0.4064" layer="20"/>
<wire x1="0" y1="29.2" x2="0" y2="0" width="0.4064" layer="20"/>
<text>NRF 2 RFM69 Breakout Board

V 1.1.0 - 01/06/2018

@author: sineverba

https://github.com/sineverba</text>
<text>SCK</text>
<text>MOSI</text>
<text>DI0</text>
<text>3V3</text>
<text>GND</text>
<text>NSS</text>
<text>MISO</text>
<text>CE</text>
</plain>
<libraries>
<library name="SparkFun-RF">
<description>&lt;h3&gt;SparkFun RF, WiFi, Cellular, and Bluetooth&lt;/h3&gt;
In this library you'll find things that send or receive RF-- cellular modules, Bluetooth, WiFi, etc.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RFM69W-XXXS2">
<description>&lt;h3&gt;Hope RF RFM69HW RF Transceiver&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://www.hoperf.com/upload/rf/RFM69HW-V1.3.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
<description>&lt;p&gt;&lt;b&gt;Generic 3216 (1206) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="2X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Personale">
<packages>
<package name="SMA90_DIP">
<description>SMA DIP Connector 90° 50 Ohm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="SparkFun-RF" package="RFM69W-XXXS2" value="RFM69HW"/>
<element name="C1" library="SparkFun-Capacitors" package="1206" value="4.7uF">
<attribute name="PROD_ID" value="CAP-10300"/>
</element>
<element name="X1" library="Personale" package="SMA90_DIP" value=""/>
<element name="JP1" library="adafruit" package="2X04" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="11"/>
<contactref element="U1" pad="9"/>
<contactref element="C1" pad="2"/>
<contactref element="X1" pad="GND1"/>
<contactref element="X1" pad="GND2"/>
<contactref element="X1" pad="GND3"/>
<contactref element="X1" pad="GND4"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="3V3">
<contactref element="U1" pad="8"/>
<contactref element="C1" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="DI0/IRQ">
<contactref element="U1" pad="2"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="NSS/CSN">
<contactref element="U1" pad="15"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="12"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="14"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="13"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="ANT">
<contactref element="U1" pad="10"/>
<contactref element="X1" pad="ANTENNA"/>
</signal>
<signal name="CE">
<contactref element="JP1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
