<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="1.27" x2="43.485" y2="1.27" width="0" layer="20"/>
<wire x1="43.485" y1="1.27" x2="43.485" y2="54.6" width="0" layer="20"/>
<wire x1="43.485" y1="54.6" x2="1.27" y2="54.6" width="0" layer="20"/>
<wire x1="1.27" y1="54.6" x2="1.27" y2="1.27" width="0" layer="20"/>
<hole x="3.81" y="52.07" drill="3.2"/>
<hole x="40.64" y="52.07" drill="3.2"/>
<hole x="40.64" y="3.81" drill="3.2"/>
<hole x="3.81" y="3.81" drill="3.2"/>
<text>FB - 07/2019</text>
</plain>
<libraries>
<library name="arduino">
<description>Arduino parts</description>
<packages>
<package name="ARDUINO_NANO">
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="C025-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="E5-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 5 mm</description>
</package>
<package name="0207/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 12 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206-BOTTOM">
<description>&lt;h3&gt;LED 1206 SMT&lt;/h3&gt;

1206, surface mount. 

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Area: 0.125" x 0.06"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="nrf24l01">
<packages>
<package name="24L01AMP">
</package>
</packages>
</library>
<library name="TDlogo">
<packages>
<package name="FB">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ARDUINO1" library="arduino" package="ARDUINO_NANO" value="ARDUINO_NANO"/>
<element name="C33" library="rcl" package="C025-024X044" value="100nF"/>
<element name="CPOL33" library="rcl" package="E5-5" value="100µ"/>
<element name="D1" library="SparkFun-LED" package="LED-1206-BOTTOM" value="Green">
<attribute name="PROD_ID" value="DIO-11076"/>
</element>
<element name="D2" library="SparkFun-LED" package="LED-1206-BOTTOM" value="Green">
<attribute name="PROD_ID" value="DIO-11076"/>
</element>
<element name="D3" library="SparkFun-LED" package="LED-1206-BOTTOM" value="Green">
<attribute name="PROD_ID" value="DIO-11076"/>
</element>
<element name="R5" library="rcl" package="0207/12" value="560"/>
<element name="R7" library="rcl" package="0207/12" value="560"/>
<element name="R8" library="rcl" package="0207/12" value="560"/>
<element name="U$2" library="nrf24l01" package="24L01AMP" value="NRF24L01AMP"/>
<element name="U$1" library="TDlogo" package="FB" value=""/>
</elements>
<signals>
<signal name="RESET2">
<contactref element="ARDUINO1" pad="28"/>
</signal>
<signal name="GND">
<contactref element="CPOL33" pad="-"/>
<contactref element="C33" pad="2"/>
<contactref element="U$2" pad="GND"/>
<contactref element="ARDUINO1" pad="4"/>
<contactref element="ARDUINO1" pad="29"/>
</signal>
<signal name="VCC">
<contactref element="ARDUINO1" pad="27"/>
<contactref element="D1" pad="A"/>
<contactref element="D2" pad="A"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$8">
<contactref element="ARDUINO1" pad="7"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="ARDUINO1" pad="8"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="ARDUINO1" pad="9"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="CPOL33" pad="+"/>
<contactref element="C33" pad="1"/>
<contactref element="ARDUINO1" pad="17"/>
<contactref element="U$2" pad="VCC"/>
</signal>
<signal name="N$3">
<contactref element="ARDUINO1" pad="12"/>
<contactref element="U$2" pad="CE"/>
</signal>
<signal name="N$4">
<contactref element="ARDUINO1" pad="13"/>
<contactref element="U$2" pad="CSN"/>
</signal>
<signal name="N$5">
<contactref element="ARDUINO1" pad="16"/>
<contactref element="U$2" pad="SCK"/>
</signal>
<signal name="N$6">
<contactref element="ARDUINO1" pad="14"/>
<contactref element="U$2" pad="MOSI"/>
</signal>
<signal name="N$7">
<contactref element="ARDUINO1" pad="15"/>
<contactref element="U$2" pad="MISO"/>
</signal>
<signal name="N$9">
<contactref element="ARDUINO1" pad="5"/>
<contactref element="U$2" pad="IRQ"/>
</signal>
<signal name="N$11">
<contactref element="R7" pad="2"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$13">
<contactref element="R8" pad="2"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="N$14">
<contactref element="R5" pad="2"/>
<contactref element="D3" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
