<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="-0.3175" y1="0.635" x2="21.5775" y2="0.635" width="0" layer="20"/>
<wire x1="21.5775" y1="0.635" x2="21.5775" y2="17.77" width="0" layer="20"/>
<wire x1="21.5775" y1="17.77" x2="-0.3175" y2="17.77" width="0" layer="20"/>
<wire x1="-0.3175" y1="17.77" x2="-0.3175" y2="0.635" width="0" layer="20"/>
<text>FB</text>
</plain>
<libraries>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
<description>SOT23-3</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="C1210">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="M1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="optocoupler">
<description>&lt;b&gt;Opto Couplers&lt;/b&gt;&lt;p&gt;
Siemens, Hewlett-Packard, Texas Instuments, Sharp, Motorola&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL04">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="TDlogo">
<packages>
<package name="FB">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BS170" library="SparkFun-DiscreteSemi" package="SOT23-3" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-00830"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl" package="C1210" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="rcl" package="C1206" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="diode" package="SOT23" value="BAT54S">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="diode" package="SOT23" value="BAT54S">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinhead" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OK1" library="optocoupler" package="DIL04" value="PC814">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="9707662"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="M1206" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="M1206" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="rcl" package="M1206" value="1.2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="I2" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="I1" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="TDlogo" package="FB" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="R3" pad="1"/>
<contactref element="BS170" pad="2"/>
<contactref element="D1" pad="1"/>
<contactref element="D2" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="VCC">
<contactref element="OK1" pad="4"/>
<contactref element="R5" pad="2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="D1" pad="2"/>
<contactref element="D2" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$13">
<contactref element="OK1" pad="1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="OK1" pad="3"/>
<contactref element="R3" pad="2"/>
<contactref element="BS170" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R6" pad="2"/>
<contactref element="I2" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="OK1" pad="2"/>
<contactref element="D2" pad="3"/>
<contactref element="I1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R5" pad="1"/>
<contactref element="BS170" pad="3"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="D1" pad="3"/>
<contactref element="A" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
