<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<description>&lt;h1&gt;PiHome - Smart Heating, Ventilation and Air Conditioning (HVAC)&lt;/h1&gt;

&lt;p&gt;nRF24L01 to RFM69CW/RFM69HCW/RFM69W/ Adapter compatible with MySensors Library&lt;/p&gt;

&lt;h4&gt;Size/Compatibility&lt;/h4&gt;

&lt;p&gt; RFM69CW/RFM69HCW/RFM69W&lt;/p&gt;

&lt;p&gt;For more information check PiHome website &lt;a href=@http://www.pihome.eu@&gt;http://www.pihome.eu&lt;/a&gt;&lt;/p&gt;</description>
<plain>
<text>Rev:0.01</text>
<text>RFM69-95 to nRF24L01</text>
<text>http://www.pihome.eu</text>
<text>PiHome</text>
<text>ANT</text>
<wire x1="0" y1="0" x2="33" y2="0" width="0.0001" layer="20"/>
<wire x1="33" y1="0" x2="33" y2="16.5" width="0.0001" layer="20"/>
<wire x1="33" y1="16.5" x2="0" y2="16.5" width="0.0001" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="16.5" width="0.0001" layer="20"/>
<text>PiHome</text>
<text>PiHome</text>
<text>http://www.pihome.eu</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="U.FL">
</package>
<package name="2X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
<library name="LowPowerLab">
<packages>
<package name="RFM12B-ANTENNA">
</package>
<package name="RFM69W-MINPADS">
</package>
</packages>
</library>
<library name="RFM69">
<packages>
<package name="RFM69">
<description>Package for Hope RF s RFM22-xxx-S2 SMD wireless transciever, xxx is module s frequency band.
*Unproven*''</description>
</package>
</packages>
</library>
<library name="SparkFun-RF">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find things that send or receive RF- GPS, cellular modules, Bluetooth, WiFi, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RFM69HCW-XXXS2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$6" library="LowPowerLab" package="RFM12B-ANTENNA" value="RFM12B_ANTENNA"/>
<element name="X2" library="adafruit" package="U.FL" value="">
<attribute name="VALUE"/>
</element>
<element name="RFM69W-433MHZ" library="LowPowerLab" package="RFM69W-MINPADS" value="RFM69"/>
<element name="RFM69CW/RFM69W" library="SparkFun-RF" package="RFM69HCW-XXXS2" value="RFM69HCW">
<attribute name="PROD_ID" value="IC-11997, IC-12053"/>
</element>
<element name="LOGO2" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
<element name="JP1" library="adafruit" package="2X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="RFM69" package="RFM69" value="RFM69SMD"/>
</elements>
<signals>
<signal name="GND">
<contactref element="RFM69W-433MHZ" pad="GND"/>
<contactref element="RFM69CW/RFM69W" pad="8"/>
<contactref element="RFM69CW/RFM69W" pad="10"/>
<contactref element="RFM69CW/RFM69W" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="U$1" pad="14"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="VCC">
<contactref element="RFM69W-433MHZ" pad="VDD"/>
<contactref element="RFM69CW/RFM69W" pad="13"/>
<contactref element="JP1" pad="2"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="D13_SCK">
<contactref element="RFM69W-433MHZ" pad="SCK"/>
<contactref element="RFM69CW/RFM69W" pad="4"/>
<contactref element="JP1" pad="5"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="D11_MOSI">
<contactref element="RFM69W-433MHZ" pad="MOSI"/>
<contactref element="RFM69CW/RFM69W" pad="3"/>
<contactref element="JP1" pad="6"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="D12_MISO">
<contactref element="RFM69W-433MHZ" pad="MISO"/>
<contactref element="RFM69CW/RFM69W" pad="2"/>
<contactref element="JP1" pad="7"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="D10_CSN">
<contactref element="RFM69W-433MHZ" pad="NSS"/>
<contactref element="RFM69CW/RFM69W" pad="5"/>
<contactref element="JP1" pad="4"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="D2_IRQ">
<contactref element="RFM69W-433MHZ" pad="DIO0"/>
<contactref element="RFM69CW/RFM69W" pad="14"/>
<contactref element="JP1" pad="8"/>
<contactref element="U$1" pad="9"/>
</signal>
<signal name="N$3">
<contactref element="U$6" pad="P$1"/>
<contactref element="X2" pad="3"/>
<contactref element="RFM69W-433MHZ" pad="ANA"/>
<contactref element="RFM69CW/RFM69W" pad="9"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="D9_CE">
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="13"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
